(footprint "SolderWire-0.25sqmm_1x05_P4.5mm_D0.65mm_OD2mm_Relief"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Soldered wire connection with feed through strain relief, for 5 times 0.25 mm² wires, reinforced insulation, conductor diameter 0.65mm, outer diameter 2mm, size source Multi-Contact FLEXI-2V 0.25 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 0.25sqmm strain-relief")
	(property "Reference" "REF**"
		(at 9 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderWire-0.25sqmm_1x05_P4.5mm_D0.65mm_OD2mm_Relief"
		(at 9 14.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 9 6 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 12)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.5 12)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 9 12)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 13.5 12)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 18 12)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "2" thru_hole circle
		(at 4.5 0)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 9 0)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 13.5 0)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 18 0)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.25sqmm_1x05_P4.5mm_D0.65mm_OD2mm_Relief.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
