(footprint "SolderWire-0.5sqmm_1x05_P4.6mm_D0.9mm_OD2.1mm_Relief"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Soldered wire connection with feed through strain relief, for 5 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 0.5sqmm strain-relief")
	(property "Reference" "REF**"
		(at 9.2 -2.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderWire-0.5sqmm_1x05_P4.6mm_D0.9mm_OD2.1mm_Relief"
		(at 9.2 15.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 9.2 6.3 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 12.6)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.6 12.6)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 9.2 12.6)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 13.8 12.6)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 18.4 12.6)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.119048)
	)
	(pad "2" thru_hole circle
		(at 4.6 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 9.2 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 13.8 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 18.4 0)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x05_P4.6mm_D0.9mm_OD2.1mm_Relief.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
