(footprint "SolderWire-2.5sqmm_1x02_P8.8mm_D2.4mm_OD4.4mm_Relief"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Soldered wire connection with feed through strain relief, for 2 times 2.5 mm² wires, reinforced insulation, conductor diameter 2.4mm, outer diameter 4.4mm, size source Multi-Contact FLEXI-xV 2.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 2.5sqmm strain-relief")
	(property "Reference" "REF**"
		(at 4.4 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderWire-2.5sqmm_1x02_P8.8mm_D2.4mm_OD4.4mm_Relief"
		(at 4.4 30.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 4.4 13.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 26.4)
		(size 4.9 4.9)
		(drill 4.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 8.8 26.4)
		(size 4.9 4.9)
		(drill 4.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 4.4 4.4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.056818)
	)
	(pad "2" thru_hole circle
		(at 8.8 0)
		(size 4.4 4.4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-2.5sqmm_1x02_P8.8mm_D2.4mm_OD4.4mm_Relief.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
