(footprint "SolderWire-2sqmm_1x04_P7.8mm_D2mm_OD3.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Soldered wire connection, for 4 times 2 mm² wires, reinforced insulation, conductor diameter 2mm, outer diameter 3.9mm, size source Multi-Contact FLEXI-xV 2.0 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 2sqmm")
	(property "Reference" "REF**"
		(at 11.7 -3.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderWire-2sqmm_1x04_P7.8mm_D2mm_OD3.9mm"
		(at 11.7 3.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 11.7 0 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3.9 3.9)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.064103)
	)
	(pad "2" thru_hole circle
		(at 7.8 0)
		(size 3.9 3.9)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 15.6 0)
		(size 3.9 3.9)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.4 0)
		(size 3.9 3.9)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-2sqmm_1x04_P7.8mm_D2mm_OD3.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
