(footprint "Wuerth_WR-PHD_610026243021_SMD_2x13_P2.54mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Connector Wuerth, WR-PHD 2.54mm Dual Socket Header Bottom Entry SMD, Wuerth electronics 610026243021 (https://katalog.we-online.de/em/datasheet/610026243021.pdf), generated with kicad-footprint-generator")
	(tags "Connector Wuerth WR-PHD 2.54mm 610026243021")
	(property "Reference" "REF**"
		(at 0 -17.71 0)
		(layer "F.SilkS")
	)
	(property "Value" "Wuerth_WR-PHD_610026243021_SMD_2x13_P2.54mm_Vertical"
		(at 0 17.91 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd rect
		(at -3.2 -15.24)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.2 -12.7)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.2 -10.16)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -3.2 -7.62)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.2 -5.08)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -3.2 -2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at -3.2 0)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at -3.2 2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at -3.2 5.08)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at -3.2 7.62)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at -3.2 10.16)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at -3.2 12.7)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd rect
		(at -3.2 15.24)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at 3.2 -15.24)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at 3.2 -12.7)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 3.2 -10.16)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at 3.2 -7.62)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at 3.2 -5.08)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at 3.2 -2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at 3.2 0)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 3.2 2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at 3.2 5.08)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 3.2 7.62)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.2 10.16)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 3.2 12.7)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd rect
		(at 3.2 15.24)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -15.24)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -12.7)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -10.16)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -7.62)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -5.08)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 0)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 5.08)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 7.62)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 10.16)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 12.7)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 15.24)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -15.24)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -12.7)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -10.16)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -7.62)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -5.08)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 0)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 5.08)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 7.62)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 10.16)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 12.7)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 15.24)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -15.81 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wuerth.3dshapes/Wuerth_WR-PHD_610026243021_SMD_2x13_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
