(footprint "Wuerth_WR-PHD_61300625721_Standard_2x03_P2.54mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Connector Wuerth, WR-PHD 2.54mm Dual Socket Header Bottom Entry Standard, Wuerth electronics 61300625721 (https://katalog.we-online.de/em/datasheet/61300625721.pdf), generated with kicad-footprint-generator")
	(tags "Connector Wuerth WR-PHD 2.54mm 61300625721")
	(property "Reference" "REF**"
		(at 2.54 -2.72 0)
		(layer "F.SilkS")
	)
	(property "Value" "Wuerth_WR-PHD_61300625721_Standard_2x03_P2.54mm_Vertical"
		(at 2.54 8 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "3" thru_hole circle
		(at 0 2.54)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "5" thru_hole circle
		(at 0 5.08)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "4" thru_hole circle
		(at 5.08 2.54)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "6" thru_hole circle
		(at 5.08 5.08)
		(size 1.3 1.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 2.54)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 5.08)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 2.54)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 5.08)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 2.54 -0.82 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wuerth.3dshapes/Wuerth_WR-PHD_61300625721_Standard_2x03_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
