(footprint "Converter_ACDC_Hi-Link_HLK-5Mxx"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ACDC-Converter, 5W, Hi-Link, HLK-5Mxx, THT (Script generated with StandardBox.py) (https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%975W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%915W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf)")
	(tags "ACDC-Converter 5W THT Hi-Link board mount module")
	(property "Reference" "REF**"
		(at -1.5 -10.79 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_Hi-Link_HLK-5Mxx"
		(at 16.8 17 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16.8 3 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 6)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 33.6 -6)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 33.6 12)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_Hi-Link_HLK-5Mxx.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
