(footprint "Converter_ACDC_MeanWell_IRM-02-xx_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ACDC-Converter, 3W, Meanwell, IRM-02, SMD, https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF")
	(tags "ACDC-Converter 3W")
	(property "Reference" "REF**"
		(at -9.18 -17.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_MeanWell_IRM-02-xx_SMD"
		(at 0 17.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -13.235 -13.97 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -13.235 -8.89 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -13.235 -3.81 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -13.235 6.35 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -13.235 8.89 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -13.235 11.43 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -13.235 13.97 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 13.235 13.97 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 13.235 11.43 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 13.235 8.89 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 13.235 6.35 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 13.235 -3.81 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 13.235 -8.89 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 13.235 -13.97 270)
		(size 1.5 2.03)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-02-xx_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
