(footprint "Converter_ACDC_MeanWell_IRM-03-xx_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT, https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF")
	(tags "ACDC-Converter 3W THT")
	(property "Reference" "REF**"
		(at 8.89 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_MeanWell_IRM-03-xx_THT"
		(at 8.89 16.24 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.89 14.24 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.3 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08)
		(size 2.3 2.3)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 30.48)
		(size 2.3 2.3)
		(drill 0.76)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 17.78 30.48)
		(size 2.3 2.3)
		(drill 0.76)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 17.78 25.4)
		(size 2.3 2.3)
		(drill 0.76)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-03-xx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
