(footprint "Converter_ACDC_MeanWell_MFM-10-xx_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AC/DC board mount open frame power converter, input 80 ~ 264 VAC, 10W output, https://www.meanwellusa.com/upload/pdf/MFM-10/MFM-10-spec.pdf")
	(tags "AC/DC power converter")
	(property "Reference" "REF**"
		(at 0 14 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_MeanWell_MFM-10-xx_THT"
		(at 20 14.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-V"
		(at 38.15 8.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "+V"
		(at 38.35 0.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "AC/N"
		(at 0.35 -2.4 0)
		(layer "F.SilkS")
	)
	(fp_text user "AC/L"
		(at 3.65 10.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 19.5 1.7 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 10.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 38.5 10.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 38.5 2.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_MFM-10-xx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
