(footprint "Converter_ACDC_MeanWell_MFM-15-xx_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AC/DC board mount open frame power converter, input 80 ~ 264 VAC, 15W output, https://www.meanwell.com/Upload/PDF/MFM-15/MFM-15-SPEC.PDF")
	(tags "AC/DC power converter")
	(property "Reference" "REF**"
		(at 0.2 23.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_MeanWell_MFM-15-xx_THT"
		(at 21.2 23.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-V"
		(at 44.5 18.6 0)
		(layer "F.SilkS")
	)
	(fp_text user "+V"
		(at 44.7 10.6 0)
		(layer "F.SilkS")
	)
	(fp_text user "AC/L"
		(at 0.35 2.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "AC/N"
		(at 0.9 18.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 24.1 10.8 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 20.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 45.05 20.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 45.05 12.75)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_MFM-15-xx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
