(footprint "Converter_ACDC_Murata_BAC05SxxDC_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ACDC-Converter, Murata, 5W, ClassB, https://www.murata.com/products/productdata/8809982558238/KAC-BAC05.pdf")
	(tags "switching power supply tht")
	(property "Reference" "REF**"
		(at 0 -4.1656 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_Murata_BAC05SxxDC_THT"
		(at 10.16 24.384 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Isolation barrier"
		(at 11.95 9.56 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 10.16 10.16 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 5.08)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 20.32 20.32)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 20.32 10.16)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 20.32 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "Isolation barrier")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 13.82 7.5) (xy 18.82 7.5) (xy 18.82 22.9) (xy 10.3 22.9) (xy 10.3 15.25) (xy 9.8 15) (xy 9.35 14.725)
				(xy 8.9 14.425) (xy 8.475 14.1) (xy 8.05 13.725) (xy 7.7 13.375) (xy 7.425 13.075) (xy 7.3 12.925)
				(xy 7.075 12.65) (xy 6.875 12.375) (xy 6.525 11.825) (xy 6.325 11.475) (xy 6.025 10.825) (xy 5.875 10.475)
				(xy 5.75 10.125) (xy 5.625 9.725) (xy 5.55 9.45) (xy 5.475 9.15) (xy 5.425 8.875) (xy 5.35 8.425)
				(xy 5.3 7.9) (xy 5.3 7.35) (xy 5.3 -2.575) (xy 13.82 -2.575)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_Murata_BAC05SxxDC_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
