(footprint "Converter_ACDC_TRACO_TMF_201xx_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ACDC-Converter, TRACO, TMF 201xx, 20W, Rev. August 28. 2024 (Script generated with StandardBox.py) (https://www.tracopower.com/products/tmf20.pdf)")
	(tags "ACDC-Converter TRACO TMF20 THT 20W")
	(property "Reference" "REF**"
		(at -2.15 -24.04 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_TRACO_TMF_201xx_THT"
		(at 23.5 24.15 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 23.5 -0.05 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 17.5)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 47 -10.05)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 47 9.95)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_TRACO_TMF_201xx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
