(footprint "Converter_ACDC_TRACO_TMF_301xx_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ACDC-Converter, TRACO, TMF 301xx, 30W, Rev. October 10. 2024 (Script generated with StandardBox.py) (https://www.tracopower.com/products/tmf30.pdf)")
	(tags "ACDC-Converter TRACO TMF30 THT 30W")
	(property "Reference" "REF**"
		(at -2.3 -24.34 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_TRACO_TMF_301xx_THT"
		(at 28.05 24.55 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 28.05 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 17.5)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 54 -10)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 54 10)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_TRACO_TMF_301xx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
