(footprint "Converter_ACDC_TRACO_TMLM-10-20_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ACDC-Converter, TRACO TMLM 10, TRACO TMLM 20, https://www.tracopower.com/products/tmlm.pdf")
	(tags "ACDC-Converter TRACO TMLM 10 and TMLM 20")
	(property "Reference" "REF**"
		(at -1.26 -15.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_ACDC_TRACO_TMLM-10-20_THT"
		(at 21.26 14.69 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 22 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 36 9.4)
		(size 4 4)
		(drill 4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.8 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 10.16)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 45.72 10.16)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 45.72 -10.16)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_TRACO_TMLM-10-20_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
