(footprint "Converter_DCDC_Artesyn_ATA_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DCDC-Converter, Artesyn, ATA Series, 3W Single and Dual Output, 1500VDC Isolation, 24.0x13.7x8.0mm https://www.artesyn.com/power/assets/ata_series_ds_01apr2015_79c25814fd.pdf https://www.artesyn.com/power/assets/trn_dc-dc_ata_3w_series_releas1430412818_techref.pdf")
	(tags "DCDC SMD")
	(property "Reference" "REF**"
		(at 0 -13.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Artesyn_ATA_SMD"
		(at 0 13.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.25 -8.89)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.25 -6.35)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.25 6.35)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.25 8.89)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 8.25 8.89)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 8.25 6.35)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 8.25 -8.89)
		(size 2.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Artesyn_ATA_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
