(footprint "Converter_DCDC_Cincon_EC6Cxx_Single_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DCDC-Converter, CINCON, EC6Cxx, single output, http://www.cincon.com/upload/media/data%20sheets/Data%20Sheet%20(DC)/C%20CASE/SPEC-EC6C-V12.pdf")
	(tags "DCDC-Converter CINCON EC6Cxx single output")
	(property "Reference" "REF**"
		(at -1 -6.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Cincon_EC6Cxx_Single_THT"
		(at 22.83 46.99 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Remote"
		(at 7.413874 0.390812 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 22.01 19.63 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 5.99948 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 15.24)
		(size 6 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 0 22.86)
		(size 6 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 45.72 5.08)
		(size 5.99948 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 45.72 15.24)
		(size 6 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 45.72 25.4)
		(size 6 2.54)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Cincon_EC6Cxx_Single_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
