(footprint "Converter_DCDC_Cyntec_MUN12AD03-SH"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.cyntec.com/upfile/products/download/Cyntec%20MUN12AD03-SH_Datasheet.pdf")
	(tags "Power Module uPOL MUN12AD03")
	(property "Reference" "REF**"
		(at 0.05 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Cyntec_MUN12AD03-SH"
		(at 0 2.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.45 -0.375)
		(size 0.75 0.1)
		(layers "F.Paste")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.375 0.3) (xy -0.375 0.3) (xy -0.375 -0.05) (xy -0.125 -0.3) (xy 0.375 -0.3)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd rect
		(at -0.45 0.375)
		(size 0.75 0.6)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at -0.3 -1.375)
		(size 0.45 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.3 1.375)
		(size 0.45 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.3 -1.375)
		(size 0.45 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.3 1.375)
		(size 0.45 0.55)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.45 -0.375)
		(size 0.75 0.6)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "" smd rect
		(at 0.45 0.375)
		(size 0.75 0.6)
		(layers "F.Paste")
		(zone_connect 0)
	)
	(pad "1" smd rect
		(at -1.6 -1.2)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.6 -0.4)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.6 0.4)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.6 1.2)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.6 1.2)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.6 0.4)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.6 -0.4)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.6 -1.2)
		(size 0.7 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 1.375)
		(size 1.2 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd custom
		(at 0 0)
		(size 1.8 1)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.9 0.75) (xy -0.9 0.75) (xy -0.9 -0.5) (xy -0.65 -0.75) (xy 0.9 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "11" smd rect
		(at 0 -1.375)
		(size 1.2 0.55)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Cyntec_MUN12AD0x-SH.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
