(footprint "Converter_DCDC_Murata_MGJ2DxxxxxxSC_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Murata MGJ2DxxxxxxSC, 19.5x9.8x12.5mm, 5.2kVDC Isolated, 2W, SIP package style, https://power.murata.com/data/power/ncl/kdc_mgj2.pdf")
	(tags "Murata MGJ2DxxxxxxSC")
	(property "Reference" "REF**"
		(at 7.62 -3.61 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Murata_MGJ2DxxxxxxSC_THT"
		(at 7.61 8.22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 2.23 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 10.16 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 12.7 0)
		(size 1.7 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 15.24 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_MGJ2DxxxxxxSC_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
