(footprint "Converter_DCDC_Murata_MYRxP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Murata MYRxP PicoBK DC/DC converter with inductor, 2x2.5mm, height 1.04mm. https://www.murata.com/en-global/products/power/nonisolated-dc-dc-converter/overview/lineup/picobk")
	(tags "PicoBK DC/DC MYRBP MYRGP MYRLP")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Murata_MYRxP"
		(at 0 2.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 270)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.95 -0.55)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -0.95 0)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at -0.95 0.55)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0 -1.263)
		(size 2.05 0.325)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0 -0.45)
		(size 0.9 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0 0.45)
		(size 0.9 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0 1.263)
		(size 2.05 0.325)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0.95 -0.55)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0.95 0)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "" smd roundrect
		(at 0.95 0.55)
		(size 0.3 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "1" smd roundrect
		(at -0.9375 -0.55 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -0.9375 0 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -0.9375 0.55 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at 0.9375 0.55 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at 0.9375 0 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at 0.9375 -0.55 270)
		(size 0.35 0.375)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at 0 -1.25 270)
		(size 0.4 2.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at 0 1.25 270)
		(size 0.4 2.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at 0 0 270)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0)
		(chamfer_ratio 0.091)
		(chamfer bottom_left)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_MYRxP.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
