(footprint "Converter_DCDC_Murata_NCS1SxxxxSC_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Murata NCS1SxxxxSC (Script generated with StandardBox.py) (https://power.murata.com/data/power/ncl/kdc_ncs1.pdf)")
	(tags "Murata NCS1SxxxxSC")
	(property "Reference" "REF**"
		(at -0.42 -4.56 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Murata_NCS1SxxxxSC_THT"
		(at 8.665 6.58 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.665 0.905 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.12 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 12.7 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 15.24 0)
		(size 1.7 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_NCS1SxxxxSC_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
