(footprint "Converter_DCDC_RECOM_R-78HB-0.5L_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DCDC-Converter, RECOM, RECOM_R-78HB-0.5L, SIP-3, Horizontally Mounted, pitch 2.54mm, package size 11.5x8.5x17.5mm^3, https://www.recom-power.com/pdf/Innoline/R-78HBxx-0.5_L.pdf")
	(tags "dc-dc recom buck sip-3 pitch 2.54mm")
	(property "Reference" "REF**"
		(at 2.54 -20.06 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_RECOM_R-78HB-0.5L_THT"
		(at 2.54 2.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 -10.25 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 2.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.5 2.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.08 0)
		(size 1.5 2.3)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78HB-0.5L_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
