(footprint "Converter_DCDC_RECOM_RPMx.x-x.0"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.recom-power.com/pdf/Innoline/RPM-6.0.pdf")
	(tags "dc-dc recom buck lga-25 pitch 2.29mm")
	(property "Reference" "REF**"
		(at 0 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_RECOM_RPMx.x-x.0"
		(at 0 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd rect
		(at -4.58 -4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.29 -4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at 0 -4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at 2.29 -4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at 4.58 -4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at -4.58 -2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd rect
		(at -2.29 -2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd rect
		(at 0 -2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at 2.29 -2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd rect
		(at 4.58 -2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd rect
		(at -4.58 0)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd rect
		(at -2.29 0)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd rect
		(at 0 0)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd rect
		(at 2.29 0)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd rect
		(at 4.58 0)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd rect
		(at -4.58 2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd rect
		(at -2.29 2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd rect
		(at 0 2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd rect
		(at 2.29 2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd rect
		(at 4.58 2.29)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd rect
		(at -4.58 4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd rect
		(at -2.29 4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd rect
		(at 0 4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd rect
		(at 2.29 4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd rect
		(at 4.58 4.58)
		(size 1.06 1.06)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
