(footprint "Converter_DCDC_Silvertel_Ag5810"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DCDC-Converter, 60W POE, Silvertel, pitch 2.54mm, package size 69.98x30x15.64mm, https://silvertel.com/images/datasheets/Ag5810-datasheet-IEEE802_3bt-Power-over-Ethernet-4-pair-PD.pdf")
	(tags "DCDC-Converter Silvertel Ag5810 single output POE")
	(property "Reference" "REF**"
		(at 0.2 -11.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Silvertel_Ag5810"
		(at 32.99 7.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 32.99 5.14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.49 -7.37)
		(size 3 3)
		(drill 3)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0.49 17.65)
		(size 3 3)
		(drill 3)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 65.49 -7.37)
		(size 3 3)
		(drill 3)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 65.49 17.65)
		(size 3 3)
		(drill 3)
		(layers "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -5.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 42.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.333909 -5.118739)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 43.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -5.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 44.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 45.33752 -5.118739)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 45.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 45.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" smd rect
		(at 45.355 -3.61)
		(size 7.75 6.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 45.355 -3.61)
		(size 7.75 6.5)
		(layers "B.Cu" "B.Mask")
	)
	(pad "2" thru_hole circle
		(at 45.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 45.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 45.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.349871 -5.118739)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 46.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.341131 -5.118739)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.355 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 47.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.353482 -6.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.355 -5.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.355 -4.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.355 -3.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.355 -2.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 48.355 -1.11)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.62)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 10.16)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 12.7)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 66.04 12.7)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 66.04 10.16)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 66.04 7.62)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 66.04 5.08)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 53.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 54.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 55.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.915359 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 56.96784 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd rect
		(at 57.48 5.015)
		(size 8 13.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 57.48 5.015)
		(size 8 13.75)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" thru_hole circle
		(at 57.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 57.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 58.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 59.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.927519 8.964875)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 -1.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 -0.015)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 0.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 1.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 2.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 3.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 4.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 5.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 6.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 7.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 9.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 60.98 10.985)
		(size 0.8 0.8)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 66.04 2.54)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 66.04 0)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 66.04 -2.54)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "Isolation")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 59.475 -1.9) (xy 52.275 -1.9) (xy 52.275 11.95) (xy 56.575 11.95) (xy 56.575 16.975) (xy 51.725 16.975)
				(xy 51.725 20.125) (xy 48.725 20.125) (xy 48.725 13.975) (xy 49.275 13.975) (xy 49.275 13.475) (xy 49.275 -4.9)
				(xy 56.475 -4.9) (xy 56.475 -9.85) (xy 59.475 -9.875)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Silvertel_Ag5810.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
