(footprint "Converter_DCDC_Silvertel_Ag99xxLP_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Converter, DCDC, Silvertel Ag9900 PoE, 1500VDC isolation, Vin 36V - 75V, 4.9W - 10W output, https://silvertel.com/images/datasheets/Ag9900M-datasheet-ultra-miniature-isolated-Power-over-Ethernet-POE-module.pdf")
	(tags "DCDC converter IEEE 802.3af")
	(property "Reference" "REF**"
		(at 5.69 -2.51 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Silvertel_Ag99xxLP_THT"
		(at 5.69 21.99 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.69 9.32 270)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 270)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "2" thru_hole circle
		(at 0 2.54 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 16.13 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 18.67 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 11.38 18.67 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 11.38 16.13 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 11.38 2.54 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 11.38 0 270)
		(size 2 2)
		(drill 1.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(name "Underside")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 4.02 -1.98) (xy 4.02 6.55) (xy 0.71 6.55) (xy 0.71 11.93) (xy 7.82 11.93) (xy 7.82 20.63) (xy 4.82 20.63)
				(xy 4.82 14.93) (xy -2.29 14.93) (xy -2.29 3.56) (xy 1.02 3.56) (xy 1.02 -1.98)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Silvertel_Ag99xxLP_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
