(footprint "Converter_DCDC_TRACO_TEC3-24xxUI_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DCDC-Converter, TRACO, TEC3-24xxUI, 3W, Rev. July 31. 2024 (Script generated with StandardBox.py) (https://www.tracopower.com/products/tec3ui.pdf)")
	(tags "DCDC-Converter TRACO TEC3UI THT SIP-8 3W")
	(property "Reference" "REF**"
		(at -4.9 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_TRACO_TEC3-24xxUI_THT"
		(at -1.6 21.79 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -1.6 8.89 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 10.16)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 12.7)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 15.24)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 17.78)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TEC3-24xxUI_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
