(footprint "Converter_DCDC_TRACO_THR40-72xxWI_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DCDC-Converter, TRACO, THR40-72xxWI, THR40-72xxxWI, 40W, Rev. November 4. 2024 (Script generated with StandardBox.py) (https://www.tracopower.com/products/thr40wi.pdf)")
	(tags "DCDC-Converter TRACO THR40WI THT 2\"x1\" 40W")
	(property "Reference" "REF**"
		(at -3.65 -4.33 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_TRACO_THR40-72xxWI_THT"
		(at 7.6 50.26 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.6 22.86 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 15.24 0)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.6 45.72)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 7.56 45.72)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 17.72 45.72)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_THR40-72xxWI_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
