(footprint "Converter_DCDC_XP_POWER_JTExxxxDxx_THT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DCDC-Converter, XP POWER, Type JTE06 Series,  Dual Output")
	(tags "DCDC-Converter XP_POWER JTE06 Dual")
	(property "Reference" "REF**"
		(at 1.99 -6.22 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_XP_POWER_JTExxxxDxx_THT"
		(at 7.95 28.81 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 9.46 0)
		(layer "F.Fab")
	)
	(pad "2" thru_hole oval
		(at 0 0)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 2.54)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 0 17.78)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 0 22.86)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 15.24 22.86)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 15.24 17.78)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 15.24 2.54)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 15.24 0)
		(size 2.5 1.5)
		(drill 0.91)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_XP_POWER_JTExxxxDxx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
