(footprint "Crystal_HC52-6mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Crystal THT HC-52/6mm, http://www.kvg-gmbh.de/assets/uploads/files/product_pdfs/XS71xx.pdf")
	(tags "THT crystalHC-49/U")
	(property "Reference" "REF**"
		(at 1.9 -2.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_HC52-6mm_Vertical"
		(at 1.9 2.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.9 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.8 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC52-6mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
