(footprint "Crystal_SMD_1210-4Pin_1.2x1.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Crystal SERIES SMD1210/4 https://ecsxtal.com/store/pdf/ECX-1048.pdf, 1.2x1.0mm^2 package")
	(tags "SMT")
	(property "Reference" "REF**"
		(at -0.125 -1.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_SMD_1210-4Pin_1.2x1.0mm"
		(at 0 1.57 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.335 -0.41 270)
		(size 0.52 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.335 0.41 270)
		(size 0.52 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.335 0.41 270)
		(size 0.52 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.335 -0.41 270)
		(size 0.52 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_1210-4Pin_1.2x1.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
