(footprint "Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm_HandSoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Crystal EuroQuartz MJ series http://cdn-reichelt.de/documents/datenblatt/B400/MJ.pdf, hand-soldering, 5.0x3.2mm^2 package")
	(tags "SMD SMT crystal hand-soldering")
	(property "Reference" "REF**"
		(at 0 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm_HandSoldering"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.325 1.425)
		(size 2.85 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.325 1.425)
		(size 2.85 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.325 -1.425)
		(size 2.85 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.325 -1.425)
		(size 2.85 1.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm_HandSoldering.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
