(footprint "Crystal_SMD_FrontierElectronics_FM206"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Watch Crystal FrontierElectronics FM206 6.0mm length 1.9mm diameter http://www.chinafronter.com/wp-content/uploads/2013/12/FM206.pdf")
	(tags "['FM206']")
	(property "Reference" "REF**"
		(at -3.02 -2.1625 90)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_SMD_FrontierElectronics_FM206"
		(at 3.02 -2.1625 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.27 -3.5)
		(size 1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.27 -3.5)
		(size 1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 3.05)
		(size 3 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_FrontierElectronics_FM206.wrl"
		(offset
			(xyz 0 0.2249999962 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
