(footprint "Crystal_SMD_MicroCrystal_MS3V-T1R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Watch Crystal MicroCrystal MS3V-T1R 5.2mm length 1.4mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/MS3V-T1R.pdf")
	(tags "['MS3V-T1R']")
	(property "Reference" "REF**"
		(at -2.07 -1.9625 90)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_SMD_MicroCrystal_MS3V-T1R"
		(at 2.07 -1.9625 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.075 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.5 -3.125)
		(size 0.6 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.5 -3.125)
		(size 0.6 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 2.475)
		(size 1.5 2.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_MS3V-T1R.wrl"
		(offset
			(xyz 0 0.3249999954 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
