(footprint "Crystal_SMD_SeikoEpson_FA128-4Pin_2.0x1.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "crystal Epson Toyocom FA-128 (https://support.epson.biz/td/api/doc_check.php?dl=brief_FA-128&lang=en), 2x1.6mm^2 package")
	(tags "SMD SMT crystal")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_SMD_SeikoEpson_FA128-4Pin_2.0x1.6mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.725 0.575)
		(size 0.95 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(pad "2" smd roundrect
		(at 0.725 0.575)
		(size 0.95 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(pad "3" smd roundrect
		(at 0.725 -0.575)
		(size 0.95 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(pad "4" smd roundrect
		(at -0.725 -0.575)
		(size 0.95 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.12)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_FA128-4Pin_2.0x1.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
