(footprint "Resonator_Murata_DSS6-3Pin_W7.0mm_H2.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Ceramic Resomator/Filter Murata DSS6, http://cdn-reichelt.de/documents/datenblatt/B400/DSN6NC51H.pdf, length*width=7.0x2.5mm^2 package, package length=7.0mm, package width=2.5mm, 3 pins")
	(tags "THT ceramic resonator filter DSS6")
	(property "Reference" "REF**"
		(at 2.5 -2.47 0)
		(layer "F.SilkS")
	)
	(property "Value" "Resonator_Murata_DSS6-3Pin_W7.0mm_H2.5mm"
		(at 2.5 2.47 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Resonator_Murata_DSS6-3Pin_W7.0mm_H2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
