(footprint "Resonator_SMD-3Pin_7.2x3.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Resomator/Filter 7.2x3.0mm, Murata CSTCC8M00G53-R0; 8MHz resonator, SMD, Farnell (Element 14) #1170435, http://www.farnell.com/datasheets/19296.pdf?_ga=1.247244932.122297557.1475167906, 7.2x3.0mm^2 package")
	(tags "SMD SMT ceramic resonator filter filter")
	(property "Reference" "REF**"
		(at 0 -2.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Resonator_SMD-3Pin_7.2x3.0mm"
		(at 0 2.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.5 0)
		(size 1.4 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 0)
		(size 1.4 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.5 0)
		(size 1.4 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Resonator_SMD-3Pin_7.2x3.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
