(footprint "Resonator_SMD_Murata_CSTCR_4.5x2x1.15mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Piezoelectric Ceramic Resonator, 4.5mm x 2mm x 1.15mm, https://www.murata.com/products/productdata/8801051639838/SPEC-CSTCR4M00G53-R0.pdf?1517839209000")
	(tags "Crystal Oscillator")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Resonator_SMD_Murata_CSTCR_4.5x2x1.15mm"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.05 -1.5)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd rect
		(at 0 -1.5 270)
		(size 0.4 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd roundrect
		(at 1.05 -1.5)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.05 0)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd rect
		(at 0 0 270)
		(size 0.4 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd roundrect
		(at 1.05 0)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.05 1.5)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd rect
		(at 0 1.5 270)
		(size 0.4 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd roundrect
		(at 1.05 1.5)
		(size 0.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Resonator_SMD_Murata_CSTCR_4.5x2x1.15mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
