(footprint "D_0201_0603Metric_Pad0.64x0.40mm_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
	(tags "diode handsolder")
	(property "Reference" "REF**"
		(at 0 -1.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_0201_0603Metric_Pad0.64x0.40mm_HandSolder"
		(at 0 1.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.68 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.4325 0)
		(size 0.458 0.36)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.4325 0)
		(size 0.458 0.36)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -0.4075 0)
		(size 0.635 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.4075 0)
		(size 0.635 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
