(footprint "D_MELF-RM10_Universal_Handsoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, Universal, MELF, RM10, Handsoldering, SMD, Thruhole,")
	(tags "Diode Universal MELF RM10 Handsoldering SMD Thruhole ")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_MELF-RM10_Universal_Handsoldering"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -2.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at -5 0)
		(size 4.5 2.7)
		(drill 1.19888
			(offset 1.1 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.0925925926)
	)
	(pad "2" thru_hole roundrect
		(at 5 0 180)
		(size 4.5 2.7)
		(drill 1.19888
			(offset 1.1 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.0925925926)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
