(footprint "D_SOD-882D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOD-882D, DFN1006D-2, body 1.0 x 0.6 x 0.4mm, pitch 0.65mm, https://assets.nexperia.com/documents/data-sheet/PESD5V0L1ULD.pdf")
	(tags "Diode SOD882D DFN1006D-2")
	(property "Reference" "REF**"
		(at 0 -1.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_SOD-882D"
		(at 0 1.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.127 -1.35 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.35 0)
		(size 0.3 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 0)
		(size 0.3 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -0.4 0)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.4 0)
		(size 0.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-882D.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
