(footprint "Infineon_SG-WLL-2-3_0.58x0.28_P0.36mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon  SG-WLL-2-3, 0.58x0.28x0.15mm, https://www.infineon.com/dgdl/Infineon-SG-WLL-2-3_SPO_PDF-Package-v02_00-EN.pdf?fileId=5546d46271bf4f9201723159ce71239d")
	(tags "Infineon WLL")
	(property "Reference" "REF**"
		(at 0 -1.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_SG-WLL-2-3_0.58x0.28_P0.36mm"
		(at 0 1.09 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.68 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.185 0)
		(size 0.21 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.4761904762)
	)
	(pad "" smd roundrect
		(at 0.185 0)
		(size 0.21 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.4761904762)
	)
	(pad "1" smd roundrect
		(at -0.185 0)
		(size 0.22 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.185 0)
		(size 0.22 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/Infineon_SG-WLL-2-3_0.58x0.28_P0.36mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
