(footprint "Nexperia_DSN0603-2_0.6x0.3mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOD962-2 silicon, leadless ultra small package; 2 terminals; 0.4 mm pitch; 0.6 mm x 0.3 mm x 0.3 mm body (https://assets.nexperia.com/documents/package-information/SOD962-2.pdf https://www.nexperia.com/packages/SOD962-2.html)")
	(tags "TVS protection diodes")
	(property "Reference" "REF**"
		(at 0 -0.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nexperia_DSN0603-2_0.6x0.3mm_P0.4mm"
		(at 0 1.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.5 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.2 0 90)
		(size 0.28 0.2)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(clearance 0.05)
	)
	(pad "2" smd rect
		(at 0.2 0 90)
		(size 0.28 0.2)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(clearance 0.05)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN0603-2_0.6x0.3mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
