(footprint "OnSemi_751EP_SOIC-4_3.9x4.725mm_P2.54mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "OnSemi 751EP SOIC, 4 Pin (https://www.onsemi.com/pdf/datasheet/mb8s-d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "OnSemi SOIC Diode_SMD OnSemi_MB8S OnSemi_SOIC4W")
	(property "Reference" "REF**"
		(at 0 -3.31 0)
		(layer "F.SilkS")
	)
	(property "Value" "OnSemi_751EP_SOIC-4_3.9x4.725mm_P2.54mm"
		(at 0 3.31 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.25 -1.27)
		(size 2.1 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(pad "2" smd roundrect
		(at -3.25 1.27)
		(size 2.1 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(pad "3" smd roundrect
		(at 3.25 1.27)
		(size 2.1 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(pad "4" smd roundrect
		(at 3.25 -1.27)
		(size 2.1 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/OnSemi_751EP_SOIC-4_3.9x4.725mm_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
