(footprint "D_A-405_P2.54mm_Vertical_KathodeUp"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
	(tags "Diode A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
	(property "Reference" "REF**"
		(at 1.27 -2.47 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_A-405_P2.54mm_Vertical_KathodeUp"
		(at 1.27 3.359 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "K"
		(at -1.9 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 1.27 -2.47 0)
		(layer "F.Fab")
	)
	(fp_text user "K"
		(at -1.9 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P2.54mm_Vertical_KathodeUp.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
