(footprint "D_DO-201AE_P5.08mm_Vertical_AnodeUp"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, DO-201AE series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9*5.3mm^2, , http://www.farnell.com/datasheets/529758.pdf")
	(tags "Diode DO-201AE series Axial Vertical pin pitch 5.08mm  length 9mm diameter 5.3mm")
	(property "Reference" "REF**"
		(at 2.54 -3.77 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_DO-201AE_P5.08mm_Vertical_AnodeUp"
		(at 2.54 3.77 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "A"
		(at 5.08 2.3 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 2.54 -3.77 0)
		(layer "F.Fab")
	)
	(fp_text user "A"
		(at 5.08 2.3 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5.08 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-201AE_P5.08mm_Vertical_AnodeUp.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
