(footprint "D_P600_R-6_P7.62mm_Vertical_AnodeUp"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, P600_R-6 series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=9.1*9.1mm^2, , http://www.vishay.com/docs/88692/p600a.pdf, http://www.diodes.com/_files/packages/R-6.pdf")
	(tags "Diode P600_R-6 series Axial Vertical pin pitch 7.62mm  length 9.1mm diameter 9.1mm")
	(property "Reference" "REF**"
		(at 3.81 -5.67 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_P600_R-6_P7.62mm_Vertical_AnodeUp"
		(at 3.81 5.67 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "A"
		(at 7.62 2.6 0)
		(layer "F.SilkS")
	)
	(fp_text user "A"
		(at 7.62 2.6 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.1 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 7.62 0)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_P600_R-6_P7.62mm_Vertical_AnodeUp.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
