(footprint "Diode_Bridge_19.0x19.0x6.8mm_P12.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single phase bridge rectifier case 19x19mm, pitch 12.7mm, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/pb1000.pdf")
	(tags "Diode Bridge PB10xx")
	(property "Reference" "REF**"
		(at 6.2 17 180)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_19.0x19.0x6.8mm_P12.7mm"
		(at 5.25 -4.25 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6 6.9 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 12.7 180)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 12.7 12.7 180)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 12.7 0 180)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_19.0x19.0x6.8mm_P12.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
