(footprint "Diode_Bridge_Comchip_SCVB-L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Three phase, Bridge, Rectifier, https://www.comchiptech.com/admin/files/product/SC35VB80S-G%20Thru506369.%20SC35VB160S-G%20RevB.pdf")
	(tags "diode module")
	(property "Reference" "REF**"
		(at -3 -6.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_Comchip_SCVB-L"
		(at 7 7.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7 5.6 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 10 5)
		(drill oval 6.7 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole roundrect
		(at -2 13.6 90)
		(size 10 5)
		(drill oval 6.7 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole roundrect
		(at 7 13.6 90)
		(size 10 5)
		(drill oval 6.7 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole roundrect
		(at 16 13.6 90)
		(size 10 5)
		(drill oval 6.7 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "5" thru_hole roundrect
		(at 14 27.2)
		(size 10 5)
		(drill oval 6.7 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_Comchip_SCVB-L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
