(footprint "Diode_Bridge_GeneSiC_KBPC_T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single phase, Bridge rectifier, 28.55x28.55mm, case KBPC_T(FP), https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1501t.pdf")
	(tags "diode module")
	(property "Reference" "REF**"
		(at -7.7 -3.8 180)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_GeneSiC_KBPC_T"
		(at 9.45 11.1 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Mounting Drill Hole"
		(at 9.48325 6.12475 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "(Screw and Washer)"
		(at 9.48325 4.92475 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "+"
		(at 2.5 -0.05 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "~"
		(at 2.675 14.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 9.45 7.55 180)
		(layer "F.Fab")
	)
	(fp_text user "-"
		(at 16.575 14.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "~"
		(at 16.625 0.525 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 9.36 3.01)
		(drill oval 7.36 1.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole roundrect
		(at 16.6 -1.5)
		(size 9.36 3.01)
		(drill oval 7.36 1.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole roundrect
		(at 16.6 16.6)
		(size 9.36 3.01)
		(drill oval 7.36 1.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole roundrect
		(at 2.3 16.6)
		(size 9.36 3.01)
		(drill oval 7.36 1.01)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_GeneSiC_KBPC_T.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
