(footprint "Diode_Bridge_GeneSiC_KBPC_W"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single phase, Bridge Rectifier, 28.55x28.55mm, case KBPC_W(WP), https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc15005w.pdf")
	(tags "diode module")
	(property "Reference" "REF**"
		(at -8 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_GeneSiC_KBPC_W"
		(at 9.05 5.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Mounting Drill Hole"
		(at 9.08325 0.92475 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "(Screw and Washer)"
		(at 9.08325 -0.27525 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "~"
		(at 16.075 -4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "~"
		(at 2.125 9.775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "-"
		(at 16.025 9.775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at 2.3 -0.025 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 9.05 2.35 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 3.22 3.22)
		(drill 1.22)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 18.1 -6.7 180)
		(size 3.22 3.22)
		(drill 1.22)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 18.1 11.4 270)
		(size 3.22 3.22)
		(drill 1.22)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 11.4 180)
		(size 3.22 3.22)
		(drill 1.22)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_GeneSiC_KBPC_W.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
